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Description automatically generated]TECHNICAL SPECIFICATION
Pickup trucks

Public Body Central Project Management Agency is carrying out a public procurement procedure for the procurement of pickup trukcs for the National Police of Ukraine (hereinafter referred to as the Beneficiary). The goods offered by the suppliers shall meet the requirements set out in his Technical Specification.
	No.
	Feature
	Technical specification requirement

	1. 
	Object of procurement

	All wheel drive pick-up trucks with enclosed cargo compartment.
* the proposed vehicle is considered to meet the procurement object if it meets the following requirements

	2. 
	Place of delivery of goods
	Kyiv, Ukraine

	3. 
	Delivery term
	No later than 6 months after the Contract enters into force

	4. 
	Vehicle‘s construction
	The vehicle must be suitable for use in territory of Ukraine without additional measures.
The gauges and read-outs of the instrument cluster must be in the metric system and the vehicle must be designed for right-hand drive (left-hand steering wheel).

	5. 
	Vehicle‘s manufacturing
	The vehicle must be new and unused (made not earlier than 2025 and with mileage of not more than 3000 km). 

	6. 
	Quantity
	14 units

	7. 
	Number of passengers (with driver)
	Minimum 3 passenger seats and 1 driver seat.

	8. 
	Vehicle type
	The vehicle must be Pick-up truck with 4 separate opening doors for driver and passengers and rear cargo bed with rear opening cargo bed gate.  

	9. 
	Vehicle’s equipment
	The vehicle must be equipped with:
· Blue flashing or rotating warning light, visible from all sides of the vehicle.
· Audible siren, controlled from inside the vehicle.

	10. 
	Gearbox type
	Manual or automatic gearbox 

	11. 
	Emission standards
	Not lower than EURO V 

	12. 
	Engine
	Diesel engine

	13. 
	Drive of the axles 
	4-wheel drive system, selectable (4WD) or constant (AWD)

	14. 
	Cargo bed cover
	Cargo bed of the vehicle must be fitted with a removable cargo bed cover, covering entire cargo bed:
· Made of rigid construction and rigid materials matching or correlating with the materials of the vehicle's bodywork.
· Fitted with top opening rear loading gate.
· Sides of the cover must be without windows, rear gate may have a window. 
· Entire structure shall be capable of being easily removed and attached.
· Height of the structure should be no lower than the height of the proposed vehicle, width not narrower than the width of the proposed vehicle.

	15. 
	Trailer towing device	

	Vehicle must be fitted with standard trailer towing hitch (50 mm ball coupling, corresponding to Class A/ ISO 1103:2007 standard or equivalent) and with 13-pin (ISO 11446 or equivalent) electrical connector for the trailer.

	16. 
	Self recovery winch
	The front of the vehicle must be fitted with a self-recovery winch:
· Powered by electric motor that is conected to the electrical system of the vehicle.
· Pulling power must be at least 4000 kg.
· Equipped with synthetic winch line not shorter than 20 m.
· Line must be equipped with attachment hook.
· Equipped with wired or vireless remote control.

	17. 
	Bodywork color
	· Vehicles should be painted in the color scheme of Police department of Ukraine. Exact color scheme and color details will be specified during execution of the contract.
· Corrosion protection must be applied to the bottom, chassis and bodywork.

	18. 
	Cabin heating and ventilation
	The vehicle must have a heating system and air conditioning

	19. 
	Tyres
	The vehicle must be:
· Fitted with a set of non-studded, tyres suitable for a wide range of on-road and off-road surfaces, as well as for winter use (M+S marked);
· Vehicle must be fitted with spare wheel with tyre, similar to tyres, fitted on the vehicle. 

	20. 
	Warranty
	The Seller or its authorized representative shall ensure the warranty service of the vehicle and the service and maintenance as provided by the manufacturer at the service center specified by the Supplier or its representative in the territory of Ukraine, and if there are no service centers of the Supplier or its representative in the specified territory, the vehicle shall be transported and returned by the Supplier at its own expense from the location of the Beneficiary's deployment to the Seller's or its representative's premises for service and maintenance.
The vehicle shall be covered by a warranty of at least 12 months or 100 000 km, whithever comes first

	21. 
	Documentation to be supplied by the Supplier together with the Goods
	Vehicle maintenance and user manual with servicing instructions in English or Ukrainian, printed, one manual for each vehicle.



NOTES:
The supplier will be required to submit with the tender documents (manufacturer's technical descriptions and/or other documents) confirming that the characteristics of the goods offered by the supplier comply with the requirements.
Where the technical specification indicates a specific model or source of supply, a specific process specific to the goods or services supplied by a particular supplier, or a trademark, patent, types, specific origin or manufacture, it shall be understood that these characteristics are indicative only and that the suppliers are free to offer an equivalent option. The supplier must demonstrate the equivalence referred to in this paragraph. 
In the event that the technical specification specifies values/parameters for a particular technical characteristic, suppliers may offer goods whose values/parameters are not inferior to those specified (goods with no inferior characteristics may be offered).
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