Annex 4 to the Procurement Terms" Tender Form"

TENDER
FOR Mobile repair workshops PROCUREMENT 

	

	(date)

	

	(location)



To the Public Institution Central Project Management Agency

1. INFORMATION ABOUT THE SUPPLIER:
	Name of supplier 
(In the case of a group of suppliers, the names of all members of the group: 
Responsible partner: 
Partner No. 1:
Partner No. 2, etc.:)
	



2. INFORMATION ON THE ECONOMIC OPERATORS ON WHOSE CAPACITY THE SUPPLIER RELIES TO MEET THE CONTRACTING AUTHORITY'S QUALIFICATION REQUIREMENTS
(to be completed if the supplier uses the capacities of other economic operators as specified in Chapter 9 of the General Part of the Procurement Conditions “Relying on the capacity of entities”)
	No.
	Name, legal entity code, address of the economic operator
	Description of the part of the subject-matter of the contract to be subcontracted

	1.
	
	

	2.
	
	



3. INFORMATION ON KNOWN SUBCONTRACTORS AND THE PARTS OF THE CONTRACT TO BE SUBCONTRACTED
(to be completed if the supplier uses sub-suppliers)
	No.
	Name, legal entity code, address of the subcontractor
	Description of the part of the subject-matter of the contract to be subcontracted

	1.
	
	

	2.
	
	



4. DETAILS OF THE MEMBERS OF THE SUPPLIER'S MANAGEMENT BOARD, SUPERVISORY BOARD

(To be completed if the supplier, which is a legal person, has a collegiate management or supervisory body member(s) or other person(s) with the right to represent or control the supplier, to take a decision on its behalf, to enter into a contract, or an accountant(s) or other person(s) with the right to draw up and sign the supplier's accounting documents (Article 46(2)(2) of the LPP).)*

	No.
	Name, surname 
	Occupation

	1
	2
	3

	
	
	

	
	
	


*This information does not need to be submitted with the proposal. The supplier will be obliged to provide this information on request of the contracting authority.
The Supplier will be required to provide documentation confirming that the persons (if any) referred to in this table do not have the grounds for exclusion provided for in Article 46(1) of the LPP.

5. PRICE OF THE TENDER
	No.
	Object of procurement

	Quantity
	Unit price [footnoteRef:2] [2:  The prices in the tender shall be rounded to two decimal places.] 

EUR excl. VAT
	Price 
EUR excl. VAT
(3x4)

	1
	2
	3
	4
	5

	5.1.
	Mobile repair workshops
	2 units
	
	

	Tender price in EUR excluding VAT (sum of values in column 5)
	

	VAT rate (to be completed if applicable)[footnoteRef:3] [3:  Goods and/or services supplied to/in Ukraine are subject to 0% tax. VAT because:
- The Goods are procured under European Union Contribution Agreement No. 7000034116 for the financing of the action “Support for Provision and Sustainability of EOD Equipment in Ukraine”. The project will be duly registered in Ukraine, and a Project Registration Card confirming its tax-exempt status will be issued by the competent Ukrainian authorities. Accordingly, the Goods procured under this action will be exempt from taxes, customs duties and other charges of a similar nature in accordance with Ukrainian law;
- if the purchased goods will be exported to Ukraine, all export procedures and documents relating to the export of the purchased goods are handled and signed by the Supplier. In this respect, the Supplier will issue an invoice at a 0% VAT rate.] 

	0

	Tender price EUR incl. VAT *[footnoteRef:4] [4:  The maximum amount of funds available for procurement is specified in clause 1.16 of the Special part of the Procurement conditions. If a tender exceeds this maximum amount (360 000,00 EUR incl. VAT), the tender will be rejected.] 

	


* This price includes all costs and all taxes (excluding costs and/or taxes related to the importation of goods).
Please note that the Supplier must submit, together with its Tender, a detailed price breakdown indicating each item comprising the procurement object, its quantity and price.

6. PROPOSED VALUES FOR THE QUALITY CRITERIA (T)
	No.
	Criterion
	Proposed value

	6.1.
	Delivery time (T) 
Supplier's proposed delivery time for the entire quantity*
	___ months**


* The delivery time offered by the supplier cannot be longer than the term specified in Clause 1.9 of the Special Part of the Procurement Conditions. If the supplier offered a longer term, his tender would be rejected.
** The supplier must indicate the proposed delivery time in months, in whole numbers. If the supplier specifies months in non-integer numbers, they will be rounded off in accordance with the procedure laid down in the Procurement Conditions.
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7. TECHNICAL AND OTHER REQUIREMENTS OF THE GOODS OFFERED BY THE SUPPLIER
	No.
	Feature
	Technical specification requirement
	The exact parameters of the offered product
(if applicable, tick the relevant boxes and / or indicate the information requested)

	Manufacturer's name, model and country of origin of the goods offered by the Supplier: _________________________________.
Please be aware that the supplier's selection of a manufacturer must evaluate the manufacturer's compliance with national security requirements, specifically whether the manufacturer has any cooperation with Russia, Belarus and other countries or territories referred to in article 92(15) of the Law on Public Procurement of the Republic of Lithuania. Additionally, once a potential winner is identified, the Contracting Authority will consult the competent authorities if the supplier or manufacturer have interests that may pose threat to national security. If a positive determination is made, the supplier will be excluded from the procurement process. For example, there have been instances where tenderers were excluded from procurement because they offered goods from Chinese manufacturers, who were deemed to have interests that may pose a threat to national security.

	1.
	Object of procurement
	All-wheel drive vehicle (mini buss or truck), with internal compartment layout for mobile mechanical and electrical workshop, suitable for repairing and supporting mechanical demining machine operations in the field and provide other mechanical assistance within the capabilities of the installed equipment. 
The vehicle must be internally equipped with storage compartments, shelves and secure boxes to organize and store all mechanical tools and equipment.
All vehicles and equipment proposed in the tender must be manufactured and configured in accordance with the requirements set out below.
	

	2.
	Place of delivery of goods
	Kyiv, Ukraine
	

	3.
	Delivery term
	No later than 7 months after the Contract enters into force
	

	4.
	Vehicle‘s construction
	The vehicle must be suitable for use in territory of Ukraine without additional measures.
The gauges and read-outs of the instrument cluster must be in the metric system, and the vehicle must be designed for right-hand drive (left-hand steering wheel).
	

	5.
	Manufacturing of the equipment
	Vehicles and all ancillary equipment must be new and unused. Used or used and refurbished vehicles or equipment cannot be offered.
All base vehicles must be of the same manufacturer and model, with the same internal layout and equipment. 
Base vehicles should be made no earlier than 2025 and with a maximum mileage of less than 5000 km.
	

	6.
	Quantity
	2 units
	

	7.
	Number of passengers (with driver)
	Minimum 2 passenger seats and 1 driver seat in the driver’s cabin of the vehicle
	

	8.
	Vehicle type
	Mobile workshop vehicle must be based on Minibus/VAN with partitioned driver’s compartment or truck with rear superstructure build as an enclosed workshop body.
Rear compartment/superstructure must be modified for transporting and storing the workshop equipment, as well as for providing a workspace for maintenance tasks. 
	

	9.
	Gross vehicle weight
	Gross vehicle weight (GVW) must not exceed 5500 kg.  
The vehicle’s payload must be sufficient to support the total weight of all workshop equipment listed in the attached List, as well as the weight of all integrated interior components, including shelves, storage boxes, drawers, and any other structural fittings installed by the supplier.
Payload must accommodate the weight of the 3-person workshop team, including the driver. The total load must be carried without compromising vehicle stability, safety, or performance under both on-road and off-road operational conditions.
	

	10.
	Gearbox type
	Manual or automatic gearbox
	

	11.
	Emission standards
	Not lower than EURO V 
	

	12.
	Engine
	Diesel engine
	

	13.
	Drive of the axles
	4-wheel drive system, selectable (4WD) or constant (AWD)
	

	14.
	Requirement for the driver’s cabin of the vehicle
	Vehicle’s driver’s cabin should have following functionalities and features:
1. Seating capacity for no less than 3 people (including driver).
2. Equipped with heating and air conditioning.
3. Equipped with not less than 1 12V DC auxiliary power outlet.
4. Equipped with not less than 1 USB power outlet.
5. Equipped with first aid kit.
	

	15.
	Requirements for the features of the mobile workshop vehicle
	Mobile workshop vehicle must have the following functionalities and features:
1. Equipped with tool kit for replacing the wheel, including lifting device.
2. Equipped with LED lighting on the sides and rear (2 lights per side and on the rear and front of the vehicle) for illuminating area of at least 20 m. around the vehicle. 
3. Fitted with standard trailer towing hitch (50 mm ball coupling, corresponding to Class A/ ISO 1103:2007 standard or equivalent) and with 13-pin (ISO 11446 or equivalent) 12 V electrical connector for the trailer.
4. Provided with at least 2 fire extinguishers, suitable for extinguishing fuel – at least 2 kg extinguisher in the driver’s compartments and at least 4 kg extinguisher in the working compartment. 
	

	16.
	Requirements for the rear working compartment
	Mobile workshop vehicle must have rear working compartment with following features: 
1. Compartment must be partitioned from the driver’s compartment by solid partition (or built as separate superstructure).
[bookmark: _Hlk204691409]2. Compartment must have at least a full-width rear door or doors, opening to the sides.  
3. Working compartment must have at least 1 dedicated workplace for using computerized equipment, equipped with desk space, suitable for computer and communication equipment, and seat/chair with adjustable height and separate working light switched on at the workplace.  
4. Working compartment must have at least 1 dedicated workplace for using mechanical equipment with work bench space and vice, suitable for the technician to work standing up and using mechanical hand tools and electric equipment.    
5. Each workplace must have not less than 2 CEE 7/3 (“Shuko” type F) 230 V electric sockets.
6. The floor of the working compartment must have nonslip surface.
7. Working compartment must have interior lighting switched on from central point and separate additional lighting for each workplace.  
8. Working compartment must have internal height of at least 180 cm in the center part and have uninterrupted passageway of this height to the rear door from the working compartment. 
9. Working compartment must be equipped with separate Heating and air conditioning (HVAC) system. 
10. HVAC system of the working compartment must be controlled from single point in the working compartment and be independent from the engine of the base vehicle and must have the capability to be powered from the outside electrical power or by the means of power generation installed/caried in the working compartment. 
11. Working compartment must have a separate extraction fan for workplace where mechanical equipment will be used to extract fumes and smoke. 
12. The internal layout of the workshop vehicle must be prepared and organized according to the attached equipment list and have designated storage location for each item. The compartment must be customized to accommodate all equipment as specified, ensuring safe, accessible, and secure storage. The arrangement must support quick deployment, weight distribution, and operational efficiency while maximizing available space.
13. All equipment storage locations must include reliable securing mechanisms to prevent any movement or falling during vehicle transit, off-road use, or sudden braking. This includes but is not limited to: fixed tie-down lashing points, lockable shelving, lockable boxes, lockable drawers, and retaining nets.
	

	17.
	Power supply of the working compartment 
	Working compartment of the mobile workshop must have following power supply:
1. Electrical systems of the working compartment including heating and air conditioning systems must be powered from the engine of the base vehicle when the engine is operating. 
1. [bookmark: _Hlk198627440]Vehicle for must be equipped with removable diesel-powered electric generator, supplying 230V 1 phase AC current at 230 V +/- 10 % 50 Hz nominal voltage for working compartment and also power for the HVAC system, interior lighting and other electrical systems.
Generator must be caried inside of the vehicle in dedicated place when not in use and unloaded for use.
1. Prime power (PRP) of the diesel generator must be not less than 5 kw. 
1. Diesel generator must be equipped with power connection cable to connect to the electrical system of the vehicle not shorter than 20 m.  
1. Mobile workshop vehicle must be equipped with uninterrupted power source (UPS) or on-board battery storage system, permanently wired in the electric supply system, and providing uninterrupted power to the workplaces and lighting in case of failure of the external power supply or generator or if other power generating systems are turned off. 
1. UPS/ Battery system must have a battery energy capacity of not less than 5 kwh.
1. Working compartment must have ability to connect to the outside power source – mains power or the mobile generator, and all systems must have the ability to be powered with external electric power from single connection point.
1. Connection to external power sources must be equipped with connection cable, not shorter than 20 m. and carried in the vehicle when not in use. 
1. Electrical system must be provided with monitoring system to monitor energy consumption and charge level of the internal batteries/UPS system.
	

	18.
	Equipment and tools installed and provided with mobile workshop vehicle
	Mobile workshop vehicle must be provided with tools/equipment in following categories:
1. Diagnostic tools:
· Digital multimeter (2 units).
· Portable network tester (suitable for LAN and wireless RF/Wi-Fi environments (1 unit).
· Portable signal analyzer (or handheld spectrum analyzer) to measure, visualize, and troubleshoot radio frequency (RF) signals directly in the field (1 unit).
· Electronic torque wrench for ½ inch sockets for range 20 to 200 Nm (1 unit).
· Torque wrench for 1 inch socket for range 200 to 1000 Nm (1 unit).
· Digital caliper with range up to 140 mm (1 unit).
· Portable battery tester for 12/24 V systems.
· OBD scanner that can scan CAN systems. 

2. Battery powered cordless tools – all provided tools must use interchangeable batteries and at least 1 battery for each tool and charging station/s for simultaneous charging of at least 2 batteries must be provided with the vehicle:
· Drill/screwdriver with set of drill bits for steel at least from 3 to 10 mm diameter (1 unit).
· Impact driver for ½ inch sockets with suitable impact socket set from 10 to 32 mm and extensions of at least 2 lengths (1 unit).
· Impact driver for ¼ inch hex bits with set of suitable bits including PH, HEX and Torx bits  (1 unit)
· Angle grinder with at least 5 cut-of discs for metal and 2 grinding discs (1 unit).
· Riveter for pop-rivets (1 unit).
· Right angle ratchet for ½ inch sockets (1 unit)..

3. Corded tools:
· Angle grinder for disc size up to 125 mm (1 unit)
· Angle grinder for disc size up to 230 mm with at least 5 suitable cut-of discs for metal (1 unit).
· Impact drill with power of at least 800 w with sets of drill bits for metal and concrete from at least 6 to 12 mm (1 unit).
· Reciprocating saw with at least 5 blades for cutting steel and 5 blades for cutting aluminum (1 unit).
· Industrial heat gun with ability to reach temperature of at least 600 C (1 unit).
· Soldering iron (1 unit).
· Soldering station suitable for electronics (1 unit).
· Corded impact wrench for 1-inch sockets with suitable impact socket set at least from 24 to 50 mm (1 unit).

4. Electrical equipment:
•	Portable Metal Inertial Gas (MIG) welder with welding gun, wires and gas cylinder (cylinder can be portable or installed in the vehicle with hose reaching to the outside of the vehicle (1 unit).
•	Portable plasma cutter, equipped with internal compressor that doesn’t require outside air supply (1 unit).
•	Portable inverter Arc welder with welding cables (1 unit);
•	Tabletop grinder with grinding stone (installed around workplace for mechanical work).
•	Portable compressor with hose of at least 10 meters with quick connect end (1 unit).
•	Industrial vacuum cleaner suitable for vacuuming dry wet environments (shop-vac type) with tank of at least 20 l(1 unit).

5.  Hand tools:
•	Set of screwdrivers (PH, HEX, SL, and Torx) (1 set).
· Ratcheting screwdriver with replaceable bits, cardan joint adaptors and extensions (1 set).
•	Set of precision screwdrivers for electronics (1 set).
•	Socket set with ½ and ¼ inch sockets, ratchets, extensions and cardan joints (1 set). 
· Set of open-end wrenches at least from 6 to 32 mm (1 set)
•	Set of combination (open end and ring) wrenches at least from 8 to 24 mm (1 set).
•	Adjustable wrench (2 units, large and small).
· Adjustable pipe wrench suitable to fitting sizes up to 50 mm (1 unit).
•	Hammer with head weight in range from 0.5 to 1 kg (1 unit).
•	Sledgehammer with head weigh in range from 3 to 5 kg (1 unit).
· Hammer with rubber or plastic head (1 unit).
•	Set of chisels suitable for metal (at least 2 units of different sizes).
•	Set of metal punches (at least 5 units of different diameters).
 •	Pliers (2 units, large and small size).
•	Needle-nose pliers (1 unit).
· Side-cut pliers (1 unit).
•	Bolt cutters (1 unit).
•	Segmented utility knives (2 units).
· Ball bearing puller suitable for bearings of external diameter of at least 100 mm (1 unit).
•	Measuring tape with at least 5 meters length (1 unit).
•	Wire stripper pliers (1 unit).
•	Wire/terminal crimper (1 unit).
•	Wire stripper pliers (1 unit).
· Hydraulic bottle jack with lifting capacity of at least 20 tones (1 unit).
•	Manual ratchet winch (come-along) with pulling capacity of at least 1000 kg (1 unit).
•	Hydraulic hose crimper suitable for crimping ends on the hydraulic hoses up to 1 inch (1 unit).

Al provided tools must have dedicated place in the mobile workshop vehicle, ensuring that the tools remains stable during transportation. 
	

	19.
	Bodywork color
	Vehicles should be painted in the color scheme of Police department of Ukraine. Exact color scheme and color details will be specified during execution of the contract.
Corrosion protection must be applied to the bottom, chassis and bodywork (manufacturer’s corrosion protection or additional coating by the supplier). 
	

	20.
	Tyres
	The vehicle must be fitted with a set of non-studded, tyres suitable for a wide range of on-road and off-road surfaces, as well as for winter use (M+S marked);
Vehicle must be fitted with spare wheel with tyre, similar to tyres, fitted on the vehicle. 
	

	21.
	Warranty
	Vehicle and all ancillary equipment and provided tools, except for consumables must be covered by a warranty of at least 12 months and at least 100,000 km, for vehicle whichever comes first.
The Seller or its authorized representative shall ensure the warranty service of the vehicle and the service and maintenance as provided by the manufacturer at the service center specified by the Supplier or its representative in the territory of Ukraine, and if there are no service centers of the Supplier or its representative in the specified territory, the vehicle shall be transported and returned by the Supplier at its own expense from the location of the Beneficiary's deployment to the Seller's or its representative's premises for service and maintenance.
	

	22.
	Documentation to be supplied by the Supplier together with the Goods
	Vehicle maintenance and user manual with servicing instructions in English or Ukrainian, printed, one manual for each vehicle must be provided.
User manual must include user and service manual/s for the internal equipment that requires manuals to be used properly (or separate manuals must be provided). 
	



Notes: 
The supplier will be required to submit with the tender documents (manufacturer's technical descriptions and/or other documents) confirming that the characteristics of the goods offered by the supplier comply with the requirements.
Where the technical specification indicates a specific model or source of supply, a specific process specific to the goods or services supplied by a particular supplier, or a trademark, patent, types, specific origin or manufacture, it shall be understood that these characteristics are indicative only and that the suppliers are free to offer an equivalent option. The supplier must demonstrate the equivalence referred to in this paragraph. 
In the event that the technical specification specifies values/parameters for a particular technical characteristic, suppliers may offer goods whose values/parameters are not inferior to those specified (goods with no inferior characteristics may be offered).

8. REQUIRED DOCUMENTS AND CONFIDENTIALITY INFORMATION
Unless otherwise specified, all documents shall be submitted with the tender by means of CPP IS:
	No.
	Document
	Does the document contain confidential information?
(Yes / No)
	Explanation of what specific information in the document is confidential and why

	1
	2
	3
	4

	1.
	The joint operating agreement (in the case of a proposal submitted by a group of economic operators)
	
	

	2.
	The power of attorney or other document authorising the submission and/or signing of the tender and other documents (if the tender is not submitted by the head of the supplier, or by the head of the members of a group of economic operators, or of subcontractors, or by the head of the economic operators on whose capacity the supplier relies)
	
	

	3.
	If the supplier uses economic operators, evidence that these resources will be available for the entire duration of the contractual obligations
	
	

	4.
	Signed ESPD in pdf format (Annex 3 "ESPD" to the Purchase Conditions). 
*A separate ESPD to be completed by:
1) supplier;
2) each member of the group of suppliers (in the case of a group of suppliers);
3) each economic operator on whose capacity the supplier relies in accordance with Article 49 of the LPP (if any) (excluding quasi-suppliers)
	
	

	5.
	Technical and / or other documents confirming the compliance of the goods offered by the supplier with the requirements of the Technical Specification
	
	

	6. 
	A detailed price breakdown indicating each item comprising the procurement object, its quantity and price.
	
	

	7.
	Other documents, if required by the Procurement Terms
	
	


9. SUPPLIER’S DECLARATION

By signing this tender, I certify that:
1. I am familiar with the procurement documents, as well as with the applicable laws of the Republic of Lithuania, sub-legislative legal acts, which regulate the procedure for conducting public procurements and which may have an impact on any relations between the contracting authority and the supplier, arising out of and/or related to this procurement;
2. I accept the conditions and procedures set out in the Procurement Terms;
3. The data and information provided in the tender documents are correct and include everything necessary for the proper performance of the contract;
4. The contract will be carried out only by persons entitled to carry out the relevant activities;
5. The tender shall be valid for the period specified in the relevant clause of Section 1 of the Special Conditions of Contract;
6. In the event of a change in the declared circumstances, I undertake to inform the Contracting Authority immediately.

10. SUPPLIER’S DECLARATION ON REQUIREMENTS RELATED TO SAFEGUARDING NATIONAL SECURITY INTERESTS

By signing this tender, I certify that:
1. The supplier, its subcontractors, the economic entities whose capacities are relied upon, or persons controlling them, and the goods offered by the supplier (including their manufacturers) do not pose a threat to the national security of the beneficiary state;
2. The supplier, the subcontractor, the economic entities whose capacities are relied upon, the manufacturer of the goods offered by the supplier (including their components, packaging) or the persons controlling them are legal persons who are not registered in the states or territories listed in paragraph 15 of Article 92 of the Law on Public Procurement;  the supplier, the subcontractor, the economic entities whose capacities are relied upon, the manufacturer of the goods offered by the supplier (including their components, packaging) or the persons controlling them are natural persons who are not permanently resident in the states or territories specified in the list provided for in paragraph 15 of Article 92 of the Law on Public Procurement or who hold citizenship of these states; the goods (including their components, packaging) do not originate or the services are not provided from the states or territories listed in paragraph 15 of Article 92 of the Law on Public Procurement; the specified entities do not have an interest likely to pose a threat to national security; I am not aware that the circumstances specified in clause 4-5 of paragraph 2 (1) of Article 45 of the Public Procurement Law exist in relation to the subjects specified in clause 1-2 of paragraph 2 (1) of Article 45 of the Law on Public Procurement. This item shall apply in the event of mobilisation, war, a state of emergency or when the Government of the Republic of Lithuania, having assessed the risk that the factors which led to the declaration of mobilisation, the imposition of martial law or a state of emergency, pose a threat to national security, has adopted a decision on the application of the provision of Paragraph 21 of Article 45 of the Law on Public Procurement; the supplier, its subcontractor, the economic operator whose capacities are relied upon, is not operating in the countries or territories referred to in the list referred to in paragraph 15 of Article 92 of the Law on Public Procurement and is not a member of, or the head of a group of economic operators any member of which operates in the countries or territories referred to in the list referred to in paragraph 15 of Article 92 of the Law on Public Procurement, another member of a management or supervisory body or any other person(s) having the right to represent or control the supplier, a subcontractor, an economic operator whose capabilities are relied upon, to take a decision on its behalf or to conclude a contract, and does not participate in the activities of groups of economic operators and/or economic operators as such.
3. the supplier I represent does not have a Russian involvement exceeding the limits laid down in Article 5k of Council Regulation (EU) No 833/2014 of 31 July 2014 concerning restrictive measures in view of the actions of Russia to destabilise the situation in Ukraine, as amended by Council Regulation (EU) No 2022/576 of 8 April 2014 on Ukraine's sanctions against Ukraine. In particular, I confirm that:
(a) the supplier I represent (and none of the members of the supplier group) is not a Russian citizen or a natural or legal person, entity or body established in Russia;
(b) the supplier I represent (and none of the members of the supplier group) is not a legal person, entity or body which is owned, directly or indirectly, by more than 50 % by an entity referred to in point (a) of this paragraph;
(c) neither I nor the company I represent is a natural or legal person, entity or body acting on behalf of, or at the direction of, an entity referred to in paragraph (a) or (b);
(d) the entities listed in points (a) to (c) are not involved as subcontractors, suppliers or entities whose capacities are relied on by the supplier represented by me where they account for more than 10% of the contract value.
4. The supplier, the sub-suppliers I have used or will use in the future, the entities whose capacities I rely on and/or will rely on, the manufacturers of goods (and their components) are not subject to international sanctions implemented in the Republic of Lithuania, as defined in the Law on International Sanctions of the Republic of Lithuania.
5. the supplier, subcontractors, and entities whose capacity are relied upon are not subject to sanctions due to the armed aggression of the Russian Federation against Ukraine and sanctions under the Law on Sanctions of Ukraine.



	(Title of the Supplier's or his authorised representative's position)
	
	(Signature*)
	
	(Name, surname)




