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Description automatically generated]TECHNICAL SPECIFICATION 
Balistic protection clothing for demining PERSONNEL
Public Body Central Project Management Agency is carrying out a public procurement procedure for the procurement of the ballistic protection clothing for demining personnel for the State Emergency Service of Ukraine (hereinafter referred to as the Beneficiary). The goods offered by the suppliers should meet the requirements set out in this Technical Specification.
	Lot I “Light demining suits”

	No.
	Feature
	Technical specification requirement

	1. 
	Object of procurement

	Light type demining suit, designed for EOD and demining and search operations, designed to protect the user against explosive hazards (excessive pressure of the shock wave, impact of fragments, exposure to heat and open flame and injuries sustained in falling) within design and certification parameters of the suits.
* the proposed suit is considered to meet the procurement object if it meets the following requirements

	2. 
	Place of delivery of goods
	Kyiv, Ukraine

	3. 
	Delivery term
	No later than 6 months after the Contract enters into force

	4. 
	Components of demining suit
	The main components of an EOD suit:
1. Upper body protection assembly (1 unit) – either solid jacket, or modular assembly consisting of vest and separate sleeves (both full sleeves or separate upper and lower arm sleeves are suitable) and shoulder protectors.
2. Lower body protection assembly (1 unit) – either solid trousers or modular assembly consisting of  shorts and separate thigh and lover leg protectors. Lover body protection assembly must be equipped with suspenders. 
3. Ballistic EOD helmet with protective visor (1 unit).

	5. 
	Condition of the demining suit
	The demining suit must be new and unworn.

	6. 
	Quantity
	100 pcs.

	7. 
	Features of the demining suits
	1. The demining suit must be designed to be used for demining and search operation and provide flexibility and mobility for the operator during demining, search and EOD tasks in standing, kneeling and prone positions
2. Demining suit protective components must be made with flexible ballistic protection material (Kevlar, Aramid fiber or similar material).
3. The demining suit must be ergonomically designed to distribute the load evenly over the operator's body. 
4. Demining suit must be equipped with front, back and sleave Velcro or similar loop material patches for attaching markings

	8. 
	Protection level of the demining suit
	1. The demining suits must have frontal chest protection of not less than V50 550 m/s based on 1.1g (.17gr) Fragment Simulating Projectile (FSP) 
2. The demining suits must have frontal protection for arms, pelvis, and upper leg of not less than V50 450 m/s based on 1.1g (.17gr) Fragment Simulating Projectile (FSP)
3. The demining suits must have rear and side protection (including back of the leg) of not less than V50 250m/s based on 1.1g (.17gr) Fragment Simulating Projectile (FSP)
4. The demining helmets and visors must have protection of not less than V50 450 m/s based on 1.1g (.17gr) Fragment Simulating Projectile (FSP)

	9. 
	Sizes of the demining suits
	EOD suit size[footnoteRef:1] requirements: [1:  International clothing size] 

· M size suit with helmet in size of 54 – 57 cm – 10 units 
· L size suit with helmet in size of 57 – 60 cm – 60 units
· XL size suit with helmet in size of 60 – 64 cm - 30 units

*In case different size metric is used by manufacturer or one size covers more than one above mentioned size requirements the bidder must provide size comparison charts and explanation to prove the compliance with the requirements. 

	10. 
	Color of the demining suits
	The main color of the demining suit is black.

	11. 
	Warranty
	All components of the demining suits and helmets must have warranty of not less than 12 months.

	12. 
	Documentation to be supplied by the Supplier together with the Goods
	Maintenance and user manual with servicing instructions in English or Ukrainian, printed, one manual for each suit and helmet must be provided. 



	Lot II “Demining vests and visors”

	No.
	Feature
	Technical specification requirement

	1. 
	Object of procurement

	Ballistic protection clothing, consisting of:
· Demining visor with headband, designed for EOD, demining and search operations, designed to protect the face area demining personnel against explosive hazards (fragmentation impact, blast and heat radiation) within design and certification parameters of the visor.
· Demining vest, designed for EOD and demining and search operations, designed to protect the upper body, neck, shoulders, groin and upper thighs of demining personnel against explosive hazards (fragmentation impact, blast and heat radiation) within design and certification parameters of the vest.
* the proposed clothing is considered to meet the procurement object if it meets the following requirements

	2. 
	Place of delivery of goods
	Kyiv, Ukraine

	3. 
	Delivery term
	No later than 6 months after the Contract enters into force

	4. 
	Construction of demining vest
	1. Demining vest can be built as single unit or as set of connectable parts and offer frontal protection for the user.
2. Demining vest must be made with flexible ballistic protection material (Kevlar, Aramid fiber or similar material).
3. Demining vest must be equipped with front and shoulder Velcro or similar loop material patches for attaching markings

	5. 
	Construction of demining visors
	1. Demining visor must be equipped with headband and hinges, that allow the visor to be lifted from the line of sight of the user. 
2. Demining visor must be made from clear and translucent rigid material (polycarbonate or synthetic material with similar properties). 

	6. 
	Condition of the ballistic protection clothing
	The ballistic protection clothing must be new and unworn/unused.

	7. 
	Quantity
	Demining visor with headband – 500 pcs.
Demining vests – 500 pcs.

	8. 
	Features of the demining vests
	1. The demining vest must be designed and suitable to be used in conjunction with a demining visor or helmet when working in standing, kneeling and prone position must provide flexibility and mobility for the operator during demining, search, and EOD tasks.
2. The demining vest must be ergonomically designed to distribute the load evenly over the operator's body. 

	9. 
	Features of the demining visors
	1. The demining visor must be designed and suitable to be used in conjunction with a demining vest or suit.
2. Demining visor must be of “one size fits all” construction, with supporting headband, adjustable to different sizes of the head. 
3. The demining visor must be ergonomically designed to securely mount on the head of the user.
4. Fabric parts of the headband must be removable and washable. 

	10. 
	Protection level of the Ballistic clothing:
	Demining vest:
The demining vest must have frontal protection of not less than V50 400m/s based on 1.1g (.17gr) Fragment Simulating Projectile (FSP)
Demining visor:
The demining visor must have protection of not less than V50 200 m/s based on 1.1g (.17gr) Fragment Simulating Projectile (FSP) and comply with IMAS 10.30 2009 or equivalent standard.

	11. 
	Sizes of the Ballistic clothing
	Demining vest size[footnoteRef:2] requirements: [2:  International clothing size] 

•	M – 112 units
•	L – 230 units
•	XL – 158 units
*In case different size metric is used by manufacturer or one size covers more than one above mentioned size requirements the bidder must provide size comparison charts and explanation to prove the compliance with the requirements. 

	12. 
	Color of the ballistic clothing
	The main color of the demining vest is black.

	13. 
	Warranty
	All components of the demining vests and visors must have warranty of not less than 12 months. 

	14. 
	Documentation to be supplied by the Supplier together with the Goods
	Maintenance and user manual with servicing instructions in English or Ukrainian, printed, one manual each vest and visor must be provided. 



NOTES:
The supplier will be required to submit with the tender documents (manufacturer's technical descriptions and/or other documents) confirming that the characteristics of the goods offered by the supplier comply with the requirements.
Where the technical specification indicates a specific model or source of supply, a specific process specific to the goods or services supplied by a particular supplier, or a trademark, patent, types, specific origin or manufacture, it shall be understood that these characteristics are indicative only and that the suppliers are free to offer an equivalent option. The supplier must demonstrate the equivalence referred to in this paragraph. 
In the event that the technical specification specifies values/parameters for a particular technical characteristic, suppliers may offer goods whose values/parameters are not inferior to those specified (goods with no inferior characteristics may be offered).
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