{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":17,"n_cols":4,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
[]
["Pirkimas: Turniketo sistemos"]
["TECHNINĖ SPECIFIKACIJA"]
[]
["Nr.","Pavadinimas","Kiekis"]
[]
["1.1.","Elektrinis turniketas","2","vnt."]
["1.1.1.","Vieno kanalo"]
["1.1.2.","Integruotas LCD ekranas"]
["1.1.3.","Automatinis (savaiminis) įrenginio testavimo režimas"]
["1.1.4.","Integruotas kompresorius"]
["1.1.5.","Laikmačio nustatymas kas 1 min, intervale ≥ (1-99) min"]
["1.1.6.","Slėgis intervale ≥ (100 - 550) mmHg, reguliavimo žingsnis ≤ 5 mmHg"]
["1.1.7.","Svoris ≤ 4 kg"]
["1.1.8.","Ličio jonų arba lygiavertės technologijos akumuliatorius, veikimo laikas be maitinimo šaltinio, ne trumpiau nei 90 min. "]
["1.1.9.","Elektros tinklas 230 V /50 Hz"]
["1.1.10.","Komplektuojama su ne mažiau 8 skirtingų ilgių mažentėmis, kurių ilgio intervalas (30 -140) ± 10 cm (2 kompl.)"]