{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":204,"n_cols":4,"rows_kept":204,"cut":false,"hidden":false,"merged":[]}
[]
["Pirkimas: Dažymo įrankiai"]
["TECHNINĖ SPECIFIKACIJA"]
[]
["Nr.","Pavadinimas","Kiekis"]
[]
["1.1.","Teptukas dažymui","120","vnt."]
["1.1.1.","Sintetiniais šereliais. Dažyti vandens pagrindo dažus ir lakus."]
["1.1.2.","Plotis 25[+-5]mm, storis 10[+-5]mm"]
["1.1.3.","Medinė arba plastikinė rankena"]
["1.1.4.","Šerelių laikiklis nerūdijančio plieno"]
["1.2.","Teptukas dažymui","120","vnt."]
["1.2.1.","Sintetiniais šereliais. Dažyti vandens pagrindo dažus ir lakus."]
["1.2.2.","Plotis 50[+-5]mm, storis 10[+-5]mm"]
["1.2.3.","Medinė arba plastikinė rankena"]
["1.2.4.","Šerelių laikiklis nerūdijančio plieno"]
["1.3.","Teptukas dažymui","60","vnt."]
["1.3.1.","Sintetiniais šereliais. Dažyti vandens pagrindo dažus ir lakus."]
["1.3.2.","Plotis 75[+-5]mm, storis 10[+-5]mm"]
["1.3.3.","Medinė arba plastikinė rankena"]
["1.3.4.","Šerelių laikiklis nerūdijančio plieno"]
["1.4.","Teptukas dažymui","50","vnt."]
["1.4.1.","Sintetiniais šereliais. Dažyti vandens pagrindo dažus ir lakus."]
["1.4.2.","Plotis 100[+-5]mm, storis 10[+-5]mm"]
["1.4.3.","Medinė arba plastikinė rankena"]
["1.4.4.","Šerelių laikiklis nerūdijančio plieno"]
["1.5.","Teptukas lakavimui","120","vnt."]
["1.5.1.","Impregnuoti, lakuoti ,medienos paviršiams. Natūralūs šereliai"]
["1.5.2.","Plotis 25[+-5]mm, storis 10[+-5]mm"]
["1.5.3.","Medinė arba plastikinė rankena"]
["1.5.4.","Šerelių laikiklis nerūdijančio plieno"]
["1.6.","Teptukas lakavimui","120","vnt."]
["1.6.1.","Impregnuoti, lakuoti ,medienos paviršiams. Natūralūs šereliai."]
["1.6.2.","Plotis 50[+-5]mm, storis 10[+-5]mm"]
["1.6.3.","Medinė arba plastikinė rankena"]
["1.6.4.","Šerelių laikiklis nerūdijančio plieno"]
["1.7.","Teptukas lakavimui","60","vnt."]
["1.7.1.","Impregnuoti, lakuoti ,medienos paviršiams. Natūralūs šereliai."]
["1.7.2.","Plotis 75[+-5]mm, storis 10[+-5]mm"]
["1.7.3.","Medinė arba plastikinė rankena"]
["1.7.4.","Šerelių laikiklis nerūdijančio plieno"]
["1.8.","Teptukas lakavimui","50","vnt."]
["1.8.1.","Impregnuoti, lakuoti ,medienos paviršiams. Natūralūs šereliai."]
["1.8.2.","Plotis 100[+-5]mm, storis 10[+-5]mm"]
["1.8.3.","Medinė arba plastikinė rankena"]
["1.8.4.","Šerelių laikiklis nerūdijančio plieno"]
["1.9.","Teptukas dažymui","20","vnt."]
["1.9.1.","Mišrūs arba natūralūs šereliai."]
["1.9.2.","Plotis 120[+-20]mm, storis 30[+-5]mm"]
["1.9.3.","Medinė arba plastikinė rankena"]
["1.9.4.","Šerelių laikiklis nerūdijančio plieno"]
["1.10.","Teptukas radiatoriams ilga lenkta rankena","100","vnt."]
["1.10.1.","Mišrūs arba natūralūs šereliai"]
["1.10.2.","Plotis 40[+-10]mm, storis 10[+-5]mm"]
["1.10.3.","Medinė arba plastikinė rankena"]
["1.10.4.","Šerelių laikiklis nerūdijančio plieno"]
["1.11.","Teptukas dažymui","20","vnt."]
["1.11.1.","Medinė arba plastikinė rankena"]
["1.11.2.","Mišrūs arba natūralūs šereliai"]
["1.11.3.","Plotis 150[+-20]mm, storis 40[+-15]mm"]
["1.11.4.","Šerelių laikiklis nerūdijančio plieno"]
["1.12.","Ergonomiška volelio rankena  ","30","vnt."]
["1.12.1.","Plotis 23 [+-2]cm "]
["1.12.2.","Vidinis naudojamo volelio skersmuo 8mm "]
["1.12.3.","Plastikinė gumuota rankena"]
["1.13.","Ergonomiška volelio rankena   ","30","vnt."]
["1.13.1.","Plotis 15 [+-3]cm, ilgis 50 [+-10]cm "]
["1.13.2.","Vidinis naudojamo volelio skersmuo 8mm "]
["1.13.3.","Plastikinė gumuota rankena"]
["1.14.","Ergonomiška volelio rankena  ","30","vnt."]
["1.14.1.","Plotis 6 [+-2]cm "]
["1.14.2.","Vidinis naudojamo volelio skersmuo 6mm "]
["1.14.3.","Plastikinė gumuota rankena"]
["1.15.","Ergonomiška volelio rankena  ","30","vnt."]
["1.15.1.","Plotis 12 [+-4]cm "]
["1.15.2.","Vidinis naudojamo volelio skersmuo 6mm "]
["1.15.3.","Plastikinė gumuota rankena"]
["1.16.","Volelis poroloninis ","80","vnt."]
["1.16.1.","Plotis 7 [+-1]cm "]
["1.16.2.","Vidinis volelio skersmuo 6mm "]
["1.17.","Volelis poroloninis","80","vnt."]
["1.17.1.","Plotis 12 [+-2]cm "]
["1.17.2.","Vidinis volelio skersmuo 6mm "]
["1.18.","Volelis poliakrilinis ","150","vnt."]
["1.18.1.","Plotis 12 [+-2]cm, plauko ilgis 10[+-4]mm "]
["1.18.2.","Vidinis volelio skersmuo 6mm "]
["1.19.","Volelis poliakrilinis ","150","vnt."]
["1.19.1.","Plotis 7 [+-2]cm, plauko ilgis 10[+-4]mm "]
["1.19.2.","Vidinis volelio skersmuo 6mm "]
["1.20.","Volelis poliakrilinis","60","vnt."]
["1.20.1.","Plotis 15 [+-2]cm, plauko ilgis 10[+-4]mm, skersmuo 35[+-5] mm "]
["1.20.2.","Vidinis volelio skersmuo 8mm "]
["1.21.","Volelis poliakrilinis ","60","vnt."]
["1.21.1.","Plotis 20 [+-2]cm, plauko ilgis 10[+-4]mm, skersmuo 35[+-5] mm "]
["1.21.2.","Vidinis volelio skersmuo 8mm "]
["1.22.","Volelis poliakrilinis","60","vnt."]
["1.22.1.","Plotis 25 [+-2]cm, plauko ilgis 10[+-4]mm, skersmuo 45[+-10] mm "]
["1.22.2.","Vidinis volelio skersmuo 8mm "]
["1.23.","Volelis veliūrinis","40","vnt."]
["1.23.1.","Plotis 15 [+-2]cm, plauko ilgis 5[+-2]mm, skersmuo 40[+-5] mm "]
["1.23.2.","Vidinis volelio skersmuo 8mm "]
["1.24.","Volelis veliūrinis","40","vnt."]
["1.24.1.","Plotis 20 [+-2]cm, plauko ilgis 5[+-2]mm, skersmuo 40[+-5] mm "]
["1.24.2.","Vidinis volelio skersmuo 8mm "]
["1.25.","Volelis veliūrinis","40","vnt."]
["1.25.1.","Plotis 25 [+-2]cm, plauko ilgis 5[+-2]mm, skersmuo 40[+-5] mm "]
["1.25.2.","Vidinis volelio skersmuo 8mm "]
["1.26.","Dažų vonelė ","40","vnt."]
["1.26.1.","Plotis: 110(+-10) mm"]
["1.26.2.","Medžiaga- plastikas "]
["1.27.","Apsauginė lipni dažymo juosta ","450","vnt."]
["1.27.1.","Plotis 50[+-1]mm, ilgis 50 [+-2] m"]
["1.27.2.","Pagrindo medžiaga: popierius,atsparumas tempimui: 33(+-2) N/cm"]
["1.27.3.","Sukibimas su plienu ne mažiau 3 N/cm"]
["1.27.4.","Bendras storis: 125(+-2) µm"]
["1.28.","Apsauginė lipni dažymo juosta ","450","vnt."]
["1.28.1.","Plotis 38[+-1]mm, ilgis 50 [+-2] m"]
["1.28.2.","Pagrindo medžiaga: popierius,atsparumas tempimui: 33(+-2) N/cm"]
["1.28.3.","Sukibimas su plienu ne mažiau 3 N/cm"]
["1.28.4.","Bendras storis: 125(+-2) µm"]
["1.29.","Apsauginė lipni dažymo juosta ","250","vnt."]
["1.29.1.","Plotis 25[+-1]mm, ilgis 50 [+-2] m"]
["1.29.2.","Pagrindo medžiaga: popierius,atsparumas tempimui: 33(+-2) N/cm"]
["1.29.3.","Sukibimas su plienu ne mažiau 3 N/cm"]
["1.29.4.","Bendras storis: 125(+-2) µm"]
["1.30.","Apsauginė plėvelė su lipnia juosta ","120","vnt."]
["1.30.1.","Rulone 15(+-1) m"]
["1.30.2.","Plotis: 2600(+-50) mm."]
["1.30.3.","Sukibimas su plienu ne mažiau 3 N/cm"]
["1.30.4.","Tinkama naudoti ant lygių, struktūrinių, jautrių paviršių"]
["1.31.","Apsauginė plėvelė su lipnia juosta ","120","vnt."]
["1.31.1.","Rulone 25(+-1) m"]
["1.31.2.","Plotis: 1400(+-50) mm."]
["1.31.3.","Sukibimas su plienu ne mažiau 3 N/cm"]
["1.31.4.","Tinkama naudoti ant lygių, struktūrinių, jautrių paviršių"]
["1.32.","Dažų vonelė ","40","vnt."]
["1.32.1.","Plotis: 260(+-10) mm"]
["1.32.2.","Medžiaga- plastikas "]
["1.33.","Teleskopinis kotas volelių rankenoms","15","vnt."]
["1.33.1.","Reguliuojamo ilgio: 100(+-30) mm - 180(+-20) mm"]
["1.33.2.","Medžiaga: aliuminis"]
["1.33.3.","Plastikinė gumuota rankena"]
["1.33.4.","Tinkantis perkamiems objektams: 1.12.;1.13.;1.14.;1.15."]
["1.34.","Volelis kampams poliamidinis","20","vnt."]
["1.34.1.","Su plastikine gumuota rankena"]
["1.34.2.","Plauko ilgis: 20(+-3) mm"]
["1.35.","Glaistymo volelis ","20","vnt."]
["1.35.1.","Su plastikine gumuota rankena"]
["1.35.2.","Plotis: 210(+-20) mm"]
["1.35.3.","Šerialiai nailoniniai arba lygiaverčiai, 16(+-2)mm aukščio."]
["1.36.","Plėvelė apsauginė uždengimui","40","vnt."]
["1.36.1.","Storis: 100(+-20) mikronų."]
["1.36.2.","Plotis: 3(+-0,2) m."]
["1.36.3.","Kiekis rulone ne mažiau 10 metrų."]
["1.36.4.","Spalva: bespalvė, skaidri"]
["1.37.","Plėvelė apsauginė uždengimui","150","vnt."]
["1.37.1.","Išmatavimai: 4(+-0,1)m x 5(+-0,1)m"]
["1.37.2.","Storis 40(+-10) mkr."]
["1.38.","Dvipusio lipnumo juosta","250","vnt."]
["1.38.1.","Plotis: 20(+-1) mm"]
["1.38.2.","Rulone 5(+-0,2) m"]
["1.38.3.","Juostos laikymo galia ne mažiau 50 kg/m."]
["1.38.4.","Bendras storis 1100(+-10) µm"]
["1.38.5.","Spalva: balta"]
["1.38.6.","Pagrindo medžiaga: PE putos"]
["1.39.","Dvipusio lipnumo juosta ","30","vnt."]
["1.39.1.","Plotis: 50(+-2) mm"]
["1.39.2.","Rulone 25(+-5) m"]
["1.39.3.","Storis: 150(+-5) mkr."]
["1.39.4.","Atsparumas tempimui: 40(+-2) N/cm"]
["1.39.5.","Spalva: skaidri, permatoma"]
["1.40.","Lipni audinio juosta","60","vnt."]
["1.40.1.","Plotis: 50(+-5)mm"]
["1.40.2.","Kiekis rulone ne mažiau 30 metrų."]
["1.40.3.","Pagrindo medžiaga: PE laminuotas audinys arba lygiavertis"]
["1.40.4.","Bendras storis: 180(+-2) µm"]
["1.40.5.","Sukibimas su plienu ne mažiau 4.3 N/cm"]
["1.40.6.","Atspari drėgmei"]
["1.41.","Plėvelė apsauginė uždengimui","40","vnt."]
["1.41.1.","Storis: 200(+-20) mikronų."]
["1.41.2.","Plotis: 3(+-0,2) m."]
["1.41.3.","Kiekis rulone ne mažiau 10 metrų."]
["1.41.4.","Spalva: juoda"]
["1.42.","Apsauginė plėvelė su lipnia juosta ","100","vnt."]
["1.42.1.","Rulone ne mažiau 20 metrų."]
["1.42.2.","Plotis: 550(+-50) mm."]
["1.42.3.","Sukibimas su plienu ne mažiau 3 N/cm"]
["1.42.4.","Tinkama naudoti ant lygių, struktūrinių, jautrių paviršių"]
["1.43.","Gruntavimo šepetys","20","vnt."]
["1.43.1.","Medinė arba plastikinė rankena"]
["1.43.2.","Šereliai sintetiniai arba naturalūs"]
["1.43.3.","Plotis: 170(+-10) mm; storis: 70(+-5)mm"]
["1.44.","Išlyginamojo sluoksnio volelis","6","vnt."]
["1.44.1.","Rankena su teleskopinio koto jungtimi"]
["1.44.2.","Skersmuo 125(+-5) mm"]
["1.44.3.","Ilgis 500(+-50) mm"]
["1.44.4.","Spyglių aukštis 35(+-5) mm"]
["1.44.5.","Volelio medžiaga plastikas (PE)"]
["1.45.","Išlyginamojo sluoksnio volelis","4","vnt."]
["1.45.1.","Rankena su teleskopinio koto jungtimi"]
["1.45.2.","Skersmuo 70(+-5) mm"]
["1.45.3.","Ilgis 210(+-20) mm"]
["1.45.4.","Spyglių aukštis 20(+-3) mm"]
["1.45.5.","Volelio medžiaga plastikas (PE)"]