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PRIME MOVERS
Public Body Central Project Management Agency is carrying out a public procurement procedure for the procurement of Prime Movers for the State Transport Special Service of Ukraine (hereinafter referred to as the Beneficiary). The goods offered by the suppliers shall meet the requirements set out in this Technical Specification.
	No.
	Feature
	Technical specification requirement

	1.
	Object of procurement
	Prime movers, designed to tow semi trailers (low-bed trailers for equipment, cargo trailers and other trailers that can be safely connected to the coupling of the prime mover).
All vehicles and equipment proposed in the tender, must be manufactured and configured in accordance with the requirements set out below. 

	2.
	Place of delivery of goods
	Kyiv region, Ukraine
The exact delivery address will be provided to the supplier during the performance of the contract.

	3.
	Delivery term
	No later than 6 months after the Contract enters into force

	4.
	Quantity 
	4 units.

	5.
	Manufacturing the equipment
	The prime movers must be new and unused. Used or used and refurbished vehicles cannot be offered.
All prime movers must be of the same manufacturer and model, equipped with same connection points and equipment.
Prime movers must be made no earlier than 2024 and with a maximum mileage of not more than 5000 km.

	6.
	Warranty
	The prime movers must be covered by a warranty of at least 12 months with no mileage limit.
The Seller or its authorized representative must ensure the warranty service of the vehicle and the service and maintenance as provided by the manufacturer at the service center specified by the Supplier or its representative in the territory of Ukraine, and if there are no service centers of the Supplier or its representative in the specified territory, the vehicle must be transported and returned by the Supplier at its own expense from the location of the Beneficiary's deployment to the Seller's or its representative's premises for service and maintenance.

	7.
	Documentation to be supplied with the prime movers
	Maintenance and user manual with servicing instructions in English or Ukrainian, printed, one manual for each prime mover must be provided. 

	8. 
	Vehicle equipment
	Prime movers must be manufactured and equipped be used for intended purpose on the territory of Ukraine without any additional equipment.
The readouts of the measuring instruments and gauges must be in the metric system (SI units) and the prime mover must be designed for right-hand traffic (left-hand steering wheel).

	9.
	Combined weight
	[bookmark: _Hlk168304253]Prime movers must be rated for Gros Combined weight (GCW) of not less than 60 000 kg. 

	10.
	Engine
	Prime mover must be equipped with diesel engine with emission standard not lower than Euro III. 

	11. 
	Gearbox type
	Prime mover must be equipped with automated manual or automatic gearbox.

	12.
	Driving axles
	Prime mover must be equipped with 2 powered rear axles in 6*4 configuration. 

	13.
	Requirement for the cabin of the prime mover. 
	Prime mover’s cabin should have the following functionalities and features:
1. Height to the top of the cabin – not more than 3500 mm from the ground surface. 
2. Seating capacity for no less than 2 people (including driver).
3. Equipped with heating and air conditioning.
4. Equipped with orange/amber rotating beacons or flashing light system, visible from the 360 degrees around the vehicle. 

	14. 
	Requirements for the features of the prime mover
	Prime mover must have the following functionalities and features:
1. Equipment and accessories for tyre inflation.
2. Tool kit for replacing the wheel, including lifting device, capable of lifting axle of the prime mover for wheel replacement.
3. Fire extinguisher weighing not less than 3 kg.
4. Be equipped with spare wheel of the same size, with the same tyre as the tyres, fitted to the prime mover. 
If the wheels and tyres are different on front and rear axles of the prime mover, prime mover must be supplied with at least 2 spare wheels  - 1 for the front axle and 1 for the rear axle. 
If the spare wheels or wheel cannot be mounted on prime mover, they must be supplied as loose components at the delivery. 
5. Be equipped with hydraulic system with hydraulic pump and hydraulic reservoir sufficient for powering the hydraulic ramp system of low-bed trailer. 
6. Be equipped with towing point for recovery – no less than 1 towing point in front of the vehicle. Towing point must be equipped with hardware (pin and/or shackle) rated for the weight of the vehicle if the hardware is required for attachment of recovery lines to the towing points.  

	15.
	Requirements for the connection of the prime mover to the semi-trailer
	Prime mover must be equipped with semi-trailer connections that have the following functionalities and features:
1. The connection between the prime mower and the semi-trailer must be through the fifth-wheel coupling on the prime mover and kingpin on the semi-trailer. Dimension of the trailer kingpin – 50 mm (2 inch). 
2. The height of the fifth wheel coupling of the prime mover must be compatible with the proposed semi-trailer and suitable for trailers in use by the end user with coupling height of 1230 mm. 
3. Electric functions and controls for trailer must be connected through the 15-pin ISO 12098 standard plug or equivalent (lighting) and 7-pin ISO 7638 standard plug or equivalent (supplementary functions – ABS, EBS). 
4. The hydraulic system of the trailer must be connected to the prime mover through the toolless quick-connect hose fittings. 
5. Prime mover must be equipped with quick-connect hoses for air supply for the trailer braking system and cables with connectors for electrical functions of the trailer. 

	16.
	Compatibility of prime mover to the semi-trailers already in use
	Prime mover must be compatible with Humbaur HTS 1000 series 3 axle low bed trailers (HTS30) in use by the end user. The electrical connections of the proposed prime mover must be compatible with the existing trailer connections, namely a 15-pin ISO 12098 standard plug for lighting and a 7-pin ISO 7638 standard plug for supplementary functions, including ABS and EBS.

	17.
	Tyres
	Prime mover must be fitted with a set of non-studded tyres suitable for a wide range of on-road and off-road surfaces, as well as for winter use.

	18.
	Color of the vehicle
	Prime mover must be painted in the following colors:
1. Cabin of the prime mover must be painted in nondescript color, corresponding to the range of vehicles in professional use – white, silver, gray, black or similar color. 
2. Frame or visible parts of the frame must be painted in black or other dark color.



NOTES:
The supplier will be required to submit with the tender documents (manufacturer's technical descriptions and/or other documents) confirming that the characteristics of the goods offered by the supplier comply with the requirements.
Where the technical specification indicates a specific model or source of supply, a specific process specific to the goods or services supplied by a particular supplier, or a trademark, patent, types, specific origin or manufacture, it shall be understood that these characteristics are indicative only and that the suppliers are free to offer an equivalent option. The supplier must demonstrate the equivalence referred to in this paragraph. 
In the event that the technical specification specifies values/parameters for a particular technical characteristic, suppliers may offer goods whose values/parameters are not inferior to those specified (goods with no inferior characteristics may be offered).
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