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Description automatically generated]TECHNICAL SPECIFICATION 
buses for transporting Shool children


	No.
	Feature
	Technical specification requirement

	1. 
	Object of procurement

	Buses, configured for the transportation of school children including passengers with disability, traveling in wheelchairs.  
Vehicle must comply with UNECE M3 vehicle category and all standards, technical requirements and safety regulations in force in Republic of Armenia, including the "Technical Regulation CU 018/2011 On the safety of wheeled vehicles" part 1.16. “Requirements for vehicles designed to transport children aged 6 to 16 years.".
*the proposed vehicle is considered to meet the procurement object if it meets the following requirements

	2. 
	Place of delivery of goods
	Yerevan, Republic of Armenia.
*Exact delivery address will be provided for the supplier in the execution of the contract. 

	3. 
	Delivery term
	No later than 10 months after the Contract enters into force

	4. 
	Vehicle‘s equipment
	The vehicle must be equipped to be used in territory of the Republic of Armenia without additional measures. The gauges and read-outs of the instrument cluster must be in the metric system, and the vehicle must be designed for right-hand drive (left-hand steering wheel).

	5. 
	Vehicle‘s manufacturing
	The vehicle must be new and unused (made no earlier than 2024 and with mileage of not more than 5000 km). 

	6. 
	Quantity
	It is intended to procure no less than 6 units (minimum quantity)[footnoteRef:1] and no more than 10 units (maximum quantity)[footnoteRef:2] [1:  This is the minimum quantity that the Contracting Authority undertakes to purchase.]  [2:  The Contracting Authority does not undertake to purchase the entire quantity. The Contracting Authority intends to purchase as many goods as can be acquired, based on the unit price (rate) offered by the supplier, without exceeding the maximum amount allocated for the procurement (EUR 770,000 including VAT), but in any case, no more than 10 units.
] 


	7. 
	Number of passengers (with driver)
	Vehicles must be fitted with following seats:
1. Not less than 21 and not more than 33 standard passenger seats suitable for children (according to Technical Regulation CU 018/2011 On the safety of wheeled vehicles" part 1.16. “Requirements for vehicles designed to transport children aged 6 to 16 years);
2. 1 seat for accompanying adult passenger;
3. 1 space for the passenger traveling in the wheelchair;
4. 1 driver seat.

	8. 
	Gearbox type
	Manual, semi-automatic or automatic gearbox

	9. 
	Engine
	Diesel engine, equipped with forced induction system (Turbocharger). 

	10. 
	Emission standards
	Not lower than EURO V 

	11. 
	Requirements for the driver and passenger compartment
	Driver and passenger compartment of the vehicle must have following functionalities and features:
1. Passenger compartment must have windows on both sides throughout the length of the vehicle.
2. If windows are fitted with opening vents, they must be not larger than 25 percent of the window area and mounted at the top part of the window. 
3. Passenger compartment must be connected with driver compartment (without solid partition between compartments).
4. Passenger compartment must have at least 2 entry and exit doors on the right side of the vehicle. 
5. Doors on the right side must have lighting for the entryways. 
6. Entryways must have steps for passengers to get into the vehicle. Single step must be not higher than 20 cm, and must have depth of at least 20 cm. 
7. If the height of the first step from the road level is more than 25 cm. vehicle must be fitted with retractable step or floorboard at the entrances.
8. Driver and passenger compartment must be equipped with heating and air conditioning system (single system with ventilation channels reaching throughout the passenger compartment or separate systems, controlled from driver position).
9. Floor of the driver and passenger compartment must be covered by wear resistant non-slip material. 
10. Interior of the vehicle must be equipped with grab handles at the access doors for easier boarding and moving through the interior. Passengers, including children, must be able to reach grab handles from the level of road surface.
11. Passenger compartment must be fitted with separate interior lighting system, controlled from the driver position. 
12. Driver from the driver’s seat must have the ability to monitor interior and exterior of the vehicle at the access doors (through mirrors or dedicated camera system). Road surface and floor of the vehicle must be visible to the driver at the area of access doors. 

	12. 
	Requirement for the seats in the driver and passenger compartment. 
	Vehicle must have seats in the following configuration:
1. No standing positions for passengers must be included in the interior layout. 
2. All seats in the vehicle must be equipped with seat belts. 
3. All seats that are designated for the children must be forward-facing. 
4. Seats must be covered with durable and washable upholstery material. 
5. For seats facing the same direction, the distance between the front surface of a seatback and the rear surface of the seatback in front of it must be at least 60 cm.
6. The width of a seat cushion must be at least 32 cm.
7. Seat back for each seat must allow for at least 17 cm of clear space to each side when measured from the center of the seat back of the at a height between 20 and 60 cm above the seat cushion.
8. For the double passenger seats, same measurements of width of seat cushion and clear space from the center are also applied for each seating position. 
9. The height of the top of seat cushion to the floor level must be from 35 to 40 cm above that floor section where passenger feet are placed. 
10. The edge of the seat facing the aisle must have an armrest or a handrail. The height of the armrest or handrail from the seat cushion must be from 16 to 20 cm. 
11. Each row of the passenger seats must have dedicated marked “STOP” request button, mounted below the window line, connected to the warning light in driver’s compartment. 

	13. 
	Requirement for the disabled access and safety systems
	Vehicle must have following disabled person access and safety systems fitted:
1. Vehicle must be equipped with electric or electromechanical wheelchair lift, mounted at the access door nearest to the dedicated space for the passenger, traveling in a wheelchair. 
2. Wheelchair lift must have a lifting capacity of not less than 300 kg. 
3. Wheelchair lift must reach the level of the road surface and provide easy access to the lift for wheelchair from that level. 
4. Wheelchair lift when not in use must lift and fold into the interior or chassis of the vehicle and not protrude outside of the door. 
5. Vehicle must be equipped with wheelchair restrain system and seat belt for passenger, traveling in the wheelchair.

	14. 
	Requirements for the features of the vehicle
	Vehicle must have following functionalities and features:
1. Vehicle must be equipped with not less than 2 fire extinguishers weighing at least 2 kg. with one within reach from the driver’s seat. 
2. Vehicle must be equipped with not less than 2 automotive first aid kits.
3. Vehicle must be equipped with microphones connected to the speaker system for interior and exterior of the vehicle in the driver’s and accompanying adult’s seating positions. 
4. Vehicle must be fitted with front white and rear fog lights, switchable from the drivers position. 
5. Vehicle must be fitted with heated rear view mirrors.
6. Vehicle must be equipped with clearly marked emergency exits (at least 1 emergency exit per side). If the emergency exits require glass breaking hammers, they should be provided with the vehicle. 
7. Vehicle must be fitted with a set of rear parking sensors and rear-view camera (can be part of the vehicle’s equipment/ multimedia system or separately permanently fitted by the supplier).  
8. Vehicle must be fitted with satellite navigation device (part of the standard equipment or installed additionally by the supplier) with the road map of the Republic of Armenia. 
9. Vehicle must provide for the luggage space of at least 0,02 m3 (20 l) per seating place. Luggage space can be on the overhead shelves, under seat baskets or rear luggage space/cargo compartment. 
10. Vehicle must be fitted with at least 1 recording video camera with feed to the driver’s position for the passenger compartment. 
11. Vehicle must have reversing signal, audible for the outside of the vehicle. 
12. Vehicle must be fitted with tachograph system.
13. Vehicle must be fitted with speed limiting device (SLD).
14. Vehicle must be fitted with a device that prevents it from moving if the entry and exit doors on the right side are open or not fully closed.

	15. 
	Bodywork color
	Vehicles must have following paint scheme:
1. Vehicles should be in yellow color, corresponding to the color scheme of the school transport.
2. Front and rear of the buss must be marked with the  Identification signs "Carriage of Children".
*Exact marking scheme will be provided for the supplier in the execution of the contract.

	16. 
	Tires
	The vehicle must be:
1. Fitted with a set of all-season tires, matching dimensions, recommended by the manufacturer, suitable for use on paved and unpaved roads and suitable for winter use.
2. Provided with spare wheel with the same tire as fitted to the vehicle. Spare wheel can be mounted in dedicated position or supplied as a loose component. 
3. Provided with tool kit for replacing the wheel, including lifting device.

	17. 
	Warranty
	The Seller or its authorized representative must ensure the warranty servicing of the vehicle at the service center specified by the Supplier or its representative in the territory of the Republic of Armenia, and if there are no service centers of the Supplier or its representative in the specified territory, the vehicle must be transported and returned by the Supplier at its own expense from the location of the Beneficiary's deployment to the Seller's or its representative's premises for service and maintenance.

The vehicle must be covered by a warranty of at least 24 months or 150 000 km whichever comes first. 

Supplier must ensure, that in the case of warranty maintenance, the entity responsible for warranty and maintenance provide initial support for the user within 48 hours and provide the warranty repair on a timeline, agreed with the end user. 

Supplier must ensure that spare parts and manufacturer’s support will be available for the proposed vehicle for the period of not less than 10 years. 

	18. 
	Documentation 
	Printed vehicle maintenance and user manual with servicing instructions in English and Armenian must be provided with the vehicle.



Notes: 
The supplier will be required to submit with the tender documents (manufacturer's technical descriptions and/or other documents) confirming that the characteristics of the goods offered by the supplier comply with the requirements.
Where the technical specification indicates a specific model or source of supply, a specific process specific to the goods or services supplied by a particular supplier, or a trademark, patent, types, specific origin or manufacture, it shall be understood that these characteristics are indicative only and that the suppliers are free to offer an equivalent option. The supplier must demonstrate the equivalence referred to in this paragraph. 
In the event that the technical specification specifies values/parameters for a particular technical characteristic, suppliers may offer goods whose values/parameters are not inferior to those specified (goods with no inferior characteristics may be offered).
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