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Description automatically generated]TECHNICAL SPECIFICATION 
Pick–up trucks FOR UKRAINE DEMINING PROJECT

Central Project Management Agency is carrying out a public procurement procedure for the procurement of pick-up trucks for Ukraine demining Project. Beneficiary of the object of procurement: the National Police of Ukraine (hereinafter referred to as the Beneficiary). The goods offered by the suppliers shall meet the requirements set out in this Technical Specification.
	No.
	Feature
	Technical specification requirement

	1. 
	Object of procurement

	All wheel drive pick-up trucks with enclosed cargo compartment.
* the proposed vehicle is considered to meet the procurement object if it meets the following requirements

	2. 
	Place of delivery of goods
	Kyiv, Ukraine. 
The exact delivery address will be provided to the supplier during the performance of the contract.

	3. 
	Delivery term
	No later than 4 months from signing of the contract.

	4. 
	Vehicle‘s construction
	The vehicle must be suitable for use in territory of Ukraine without additional measures.
The gauges and read-outs of the instrument cluster must be in the metric system and the vehicle must be designed for right-hand drive (left-hand steering wheel).

	5. 
	Vehicle‘s manufacturing
	The vehicle must be new and unused (made not earlier than 2023 and with mileage of not more than 3000 km). 

	6. 
	Quantity
	11 pcs.

	7. 
	Number of passengers (with driver)
	Minimum 3 passenger seats and 1 driver seat.

	8. 
	Vehicle type
	The vehicle must be:
· Pick-up truck with 4 separate opening doors for driver and passengers.
· Cargo compartment must be covered by rigid cover, not lower than roof of passenger cabin, and not narover than cargo bed of the vehicle with openable door on the back. 

	9. 
	Vehicle’s equipment
	The vehicle must be equipped with:
· Not less than 1 blue priority lighting system (rotating or flashing), visible from all sides of the vehicle.
· Audible siren, controlled from inside the vehicle.

	10. 
	Gearbox type
	Manual or automatic gearbox 

	11. 
	Emission standards
	Not lower than EURO IV 

	12. 
	Engine
	Diesel engine

	13. 
	Drive of the axles 
	4-wheel drive system, selectable (4WD) or constant (AWD)

	14. 
	Bodywork color
	· Vehicles should be painted in the color scheme of Police department of Ukraine. Exact color scheme and color details will be specified during execution of the contract.
· Corrosion protection must be applied to the bottom, chassis and bodywork.

	15. 
	Cabin heating and ventilation
	The vehicle must have a heating system and air conditioning

	16. 
	Tyres
	The vehicle must be:
· Fitted with a set of non-studded, tyres suitable for a wide range of on-road and off-road surfaces, as well as for winter use (M+S marked);
· Vehicle must be fitted with spare wheel with tyre, similar to tyres, fitted on the vehicle. 

	17. 
	Warranty
	The Seller or its authorized representative shall ensure the warranty servicing of the vehicle at the service center specified by the Supplier or its representative in the territory of Ukraine, and if there are no service centers of the Supplier or its representative in the specified territory, the vehicle shall be transported and returned by the Supplier at its own expense from the location of the Beneficiary's deployment to the Seller's or its representative's premises for service and maintenance.
The vehicle shall be covered by a warranty of at least 12 months with no mileage limit.

	18. 
	Documentation to be supplied by the Supplier together with the Goods
	Vehicle maintenance and user manual with servicing instructions in English or Ukrainian, printed, one manual for each vehicle.



NOTES:
Where the technical specification indicates a specific model or source of supply, a specific process specific to the goods or services supplied by a particular supplier, or a trademark, patent, types, specific origin or manufacture, it shall be understood that these characteristics are indicative only and that the suppliers are free to offer an equivalent option. The supplier must demonstrate the equivalence referred to in this paragraph. 
In the event that the technical specification specifies values/parameters for a particular technical characteristic, suppliers may offer goods whose values/parameters are not inferior to those specified (goods with no inferior characteristics may be offered).
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