{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":19,"n_cols":4,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
[]
["Pirkimas: Glikolis, vandens minkštinimo druska"]
["TECHNINĖ SPECIFIKACIJA"]
[]
["Nr.","Pavadinimas","Kiekis"]
[]
["1.1.","Druska vandens minkštinimui","30000","kg"]
["1.1.1.","NaCl druska tabletėmis"]
["1.1.2.","Pakuotė atspari drėgmei."]
["1.1.3.","Įpakavimas po 25 (+-5) kg"]
["1.1.4.","Grynasis medžiagos kiekis ne mažiau kaip 99,5 %"]
["1.2.","Glikolis, neužšąlantis šildymo sistemos skystis","600","I"]
["1.2.1.","Neužšąlantis šildymo sistemos skystis paruoštas naudojimui"]
["1.2.2.","Įpakavimas: pakuotė po  20 (+-5) L"]
["1.2.3.","Šilumos nešiklis neužšąla iki -20˚C temperatūroje;"]
["1.2.4.","Virimo temperatūra ne žemesnė kaip 120˚C;"]
["1.3.","Glikolio ( neužšąlančio šildymo sistemos skysčio) koncentratas","300","I"]
["1.3.1.","Neužšąlančio šildymo sistemos skysčio koncentratas ( propilenglikolis)"]
["1.3.2.","Įpakavimas: pakuotė po 20 (+-5) L"]