{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":68,"n_cols":4,"rows_kept":68,"cut":false,"hidden":false,"merged":[]}
[]
["Pirkimas: Chirurginiai instrumentai"]
["TECHNINĖ SPECIFIKACIJA"]
[]
["Nr.","Pavadinimas","Kiekis"]
[]
["1.","Chirurginiai instrumentai"]
["1.1.","Žirklės","20","vnt."]
["1.1.1.","Žarnyno (enterotomy) žirklės"]
["1.1.2.","Tiesios"]
["1.1.3.","Viena kerpančioji dalis prailginta užapvalintu lašo formos galu, kita dalis buka"]
["1.1.4.","Bendras instrumento ilgis 215 mm ± 3 mm"]
["1.2.","Žirklės","20","vnt."]
["1.2.1.","Busch tipo arba lygiavertės bambinės žirklės"]
["1.2.2.","Lenktos"]
["1.2.3.","Bukos"]
["1.2.4.","Ilgis 160 mm ± 3 mm"]
["1.3.","Žirklės","15","vnt."]
["1.3.1.","Standard tipo arba lygiavertės chirurginės žirklės"]
["1.3.2.","bukos"]
["1.3.3.","Ilgis 130 mm ± 3 mm"]
["1.4.","Žirklės","15","vnt."]
["1.4.1.","Doyen tipo arba lygiavertės ginekologinės žirklės"]
["1.4.2.","Tiesios"]
["1.4.3.","Buki galai"]
["1.4.4.","Ilgis 185 mm ± 3 mm"]
["1.5.","Žirklės","1","vnt."]
["1.5.1.","Mayo-Stille Standard tipo arba lygiavertės preparavimo žirklės"]
["1.5.2.","Tiesios"]
["1.5.3.","Ilgis 150 mm ± 3 mm"]
["1.6.","Pincentas","10","vnt."]
["1.6.1.","Potts-Smith Normal Profile tipo arba lygiavertis disekcinis pincetas"]
["1.6.2.","Su volframo karbidu"]
["1.6.3.","Rankena spalviškai žymėta"]
["1.6.4.","Bendras instrumento ilgis 145 mm ± 3 mm"]
["1.7.","Hemostatinis spaustukas","10","vnt."]
["1.7.1.","De Bakey-Pean tipo arba lygiavertis atraumatinis spaustukas"]
["1.7.2.","Tiesus"]
["1.7.3.","Ilgis 165 mm ± 3 mm"]
["1.8.","Spaustukas","10","vnt."]
["1.8.1.","Gross-Maier tipo arba lygiavertis spaustukas"]
["1.8.2.","Tiesus"]
["1.8.3.","Rankenos su užraktu"]
["1.8.4.","Bendras instrumento ilgis 265 mm ± 3 mm"]
[]
["2.","Oftalmologiniai instrumentai"]
["2.1.","Žirklės","1","vnt."]
["2.1.1.","H.-R. KOCH modelio arba lygiavertės kapsulės žirklės"]
["2.1.2.","Horizontalios"]
["2.1.3.","Lenktos 45° ± 1° kampu"]
["2.1.4.","Ašmenys 2,5 mm ± 0,3 mm"]
["2.1.5.","≥ 360° pasukama galvutė"]
["2.1.6.","22 G dyžio / 0,7 ± 0,03 mm tiesus kotelis"]
["2.1.7.","Bendras instrumento ilgis 110 mm ± 5 mm"]
["2.1.8.","Instrumento paviršius papildomai padengtas chromu"]
["2.2.","Laipsnių matuoklis","1","vnt."]
["2.2.1.","Skirtas toriniams IOL lęšiams"]
["2.2.2.","Su ≤ 5° žingsniais ir besisukančiais išlygiavimo žiedais"]
["2.2.3.","12 ± 1 mm vidinis skersmuo"]
["2.2.4.","Bendras instrumento ilgis 110 mm ± 5 mm"]
["2.2.5.","Rankenėlė plokščia, grublėtu paviršiumi"]
["2.2.6.","Instrumento paviršius papildomai padengtas chromu"]
["2.3.","Pincetas","3","vnt."]
["2.3.1.","H.-R. KOCH modelio arba lygiavertis mikrochiruginis kapsulės pincetas"]
["2.3.2.","22 G dydžio / 0.7 ± 0,03 mm"]
["2.3.3.","Lenktas darbinis antgalis su mikro sugriebimo galiukais"]
["2.3.4.","6 mm ±1 mm titaninė rankena, veikianti paspaudimo principu"]
["2.3.5.","Bendras instrumentu ilgis 145 mm ± 5 mm"]